The client side talks to the server through fifo pipes. The client uses the “request” pipe to send messages to the server and the “reply” pipe to receive. The server uses the “reply” pipe to send messages from the client and the “request” pipe to receive messages.